IFC building model
Schema: "IFC4"
Description: "ViewDefinition[DesignTransferView]"
File name: "Inim_FA100.ifc"
Time stamp: "2026-06-29T11:38:09+03:00"
Preprocessor: "IfcOpenShell 0.8.5"
Originating system: "Bonsai 0.8.5"
Authorization: "Nobody"

Units
  VOLUMEUNIT: CUBIC_METRE
  LENGTHUNIT: METRE
  AREAUNIT: SQUARE_METRE

Spatial structure
IFCPROJECT "My Project"
  IFCSITE "My Site"
    IFCBUILDING "My Building"
      IFCBUILDINGSTOREY "My Storey"
        contains 1 element
          1 x IFCSENSOR | names: "Inim_FA100_Body" | property sets: Pset_FireDetection

Property sets
  Pset_FireDetection | properties | on 1 object (1 IFCSENSOR)
    Channels = "2" (IFCLABEL)
    Current = "400 mA" (IFCLABEL)
    Description = "Aspirating smoke detector for fire detection systems" (IFCLABEL)
    DetectionType = "Aspirating smoke detection" (IFCLABEL)
    IPRating = "IP30" (IFCLABEL)
    Manufacturer = "Inim Electronics" (IFCLABEL)
    Model = "FA100" (IFCLABEL)
    ProductType = "Aspirating Smoke Detector" (IFCLABEL)
    SamplingPipeDiameter = "25 mm" (IFCLABEL)
    Standard = "EN54-20" (IFCLABEL)
    Voltage = "24 V DC" (IFCLABEL)
    Weight = "1.95 kg" (IFCLABEL)